DATATYPE = CDS STUDY DEFINITION
FILENAME = int_dist_18.def
INSTRUME = CDS
DATE_CRE = 1997/02/12 18:14:28
END

LINELIST
    LL_ID    = 171
    DETECTOR = N
    LL_DESC  = Intensity distribution selection
    N_LINES  = 10
    LL_IND   = 1
        LINENAME = Mg VIII
        WAVELNTH = 313.754
        GR_ORDER = 1
        CEN_PIX  = 88
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = O III
        WAVELNTH = 525.796
        GR_ORDER = 1
        CEN_PIX  = 109
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Si VIII
        WAVELNTH = 319.826
        GR_ORDER = 1
        CEN_PIX  = 175
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = New VDS line
        WAVELNTH = 554.475
        GR_ORDER = 1
        CEN_PIX  = 355
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Mg X
        WAVELNTH = 625.161
        GR_ORDER = 1
        CEN_PIX  = 958
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 236
    DETECTOR = N
    DW_DESC  = Background,  10 lines. {149}  dex = (25,120) pixels <15134>
    W_WIDTH  = 25
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 171
    N_WINS   = 14
    DW_IND   = 1
        WIN_NAME = Mg_8_313_75                             
        WIN_DEF  = (76,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_3_525_80                              
        WIN_DEF  = (97,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Si_8_319_83                             
        WIN_DEF  = (163,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_554_47                               
        WIN_DEF  = (343,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (414,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (598,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (796,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (850,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_10_625_16                            
        WIN_DEF  = (946,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (985,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 8
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(60,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 8
    RAS_VAR  = 23
    RV_DESC  = (240x240) arcsec, 40s <QUIET>  Comp. 2 IDs-(171,236)
    EXPTIME  = 40
    LL_ID    = 171
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 236
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 2699
    USABLE   = Y

STUDY
    STUDY_ID = 8
    TITLE_ID = 329
    OBS_PROG = INT_DIST
    TITLE    = STUDY OF INTENSITY DISTRIBUTIONS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 8
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 8
    TITLE_ID = 329
    STUDYVAR = 18
    SV_DESC  = V1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 2699
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 8
        RAS_VAR  = 23
        N_REPEAT_R = 1
