DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/young/cds/new_studies/lifebp_1_25.def
INSTRUME = CDS
DATE_CRE = 2005/09/23 10:08:53
END

LINELIST
    LL_ID    = 478
    DETECTOR = N
    LL_DESC  = JOP 182 - strong lines (D. Bewsher, RAL)
    N_LINES  = 8
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.665
        GR_ORDER = 1
        CEN_PIX  = 78
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ca X
        WAVELNTH = 558.25
        GR_ORDER = 1
        CEN_PIX  = 400
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.3
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O III
        WAVELNTH = 599.6
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XVI
        WAVELNTH = 360.8
        GR_ORDER = 1
        CEN_PIX  = 765
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Mg IX
        WAVELNTH = 368.1
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = O V
        WAVELNTH = 629.388
        GR_ORDER = 1
        CEN_PIX  = 1007
        WAVEBAND = 2

DATAWIN
    DW_ID    = 615
    DETECTOR = N
    DW_DESC  = Background,   8 lines. {0}  dex = (35,120) pixels <37769>
    W_WIDTH  = 35
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 478
    N_WINS   = 12
    DW_IND   = 1
        WIN_NAME = Si_12_520_66                            
        WIN_DEF  = (61,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ca_10_558_25                            
        WIN_DEF  = (383,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_30                             
        WIN_DEF  = (606,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (736,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_16_360_80                            
        WIN_DEF  = (748,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_9_368_10                             
        WIN_DEF  = (851,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (952,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = O_5_629_39                              
        WIN_DEF  = (990,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 13
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(15,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 15
    NY       = 1

RASTER_VAR
    RAS_ID   = 13
    RAS_VAR  = 27
    RV_DESC  = (60x240) arcsec, 30s <QUIET>  Comp. (8,2) IDs-(478,615)
    EXPTIME  = 30
    LL_ID    = 478
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 615
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 558
    USABLE   = Y

STUDY
    STUDY_ID = 13
    TITLE_ID = 650
    OBS_PROG = LIFEBP_1
    TITLE    = LIFETIME OF X-RAY BRIGHT POINTS - RASTER
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 13
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 13
    TITLE_ID = 650
    STUDYVAR = 25
    SV_DESC  = VAR.1, 60X240, 4X240, 30S, TEMP LINES
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 558
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 13
        RAS_VAR  = 27
        N_REPEAT_R = 1
