DATATYPE = CDS STUDY DEFINITION
FILENAME = o_hivel_13.def
INSTRUME = CDS
DATE_CRE = 1996/03/11 16:39:15
END

LINELIST
    LL_ID    = 7
    DETECTOR = N
    LL_DESC  = Dynamic Line Selection
    N_LINES  = 9
    LL_IND   = 1
        LINENAME = HE  1  584.3
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O   3  599.6
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 738
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O   4  554.5
        WAVELNTH = 554.52
        GR_ORDER = 1
        CEN_PIX  = 353
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = NE  6  562.8
        WAVELNTH = 562.83
        GR_ORDER = 1
        CEN_PIX  = 424
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = MG  8  313.7
        WAVELNTH = 313.73
        GR_ORDER = 1
        CEN_PIX  = 114
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = MG  9  368.1
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 864
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = FE 13  320.8
        WAVELNTH = 320.8
        GR_ORDER = 1
        CEN_PIX  = 211
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = FE 14  334.2
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = FE 16  335.4
        WAVELNTH = 335.4
        GR_ORDER = 1
        CEN_PIX  = 413
        WAVEBAND = 1

DATAWIN
    DW_ID    = 20
    DETECTOR = N
    DW_DESC  = Background,   9 lines.  dex = (15,15) pixels <13069>
    W_WIDTH  = 15
    W_HEIGHT = 15
    VDS_BACK = 1
    LL_ID    = 7
    N_WINS   = 13
    DW_IND   = 1
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (601,445,15,15)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (731,445,15,15)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_4_554_52                              
        WIN_DEF  = (346,445,15,15)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ne_6_562_83                             
        WIN_DEF  = (417,445,15,15)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_8_313_73                             
        WIN_DEF  = (107,565,15,15)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (857,565,15,15)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Fe_13_320_80                            
        WIN_DEF  = (204,565,15,15)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (389,565,15,15)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Fe_16_335_40                            
        WIN_DEF  = (406,565,15,15)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 1
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(15,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 15
    NY       = 1

RASTER_VAR
    RAS_ID   = 1
    RAS_VAR  = 5
    RV_DESC  = (30x30) arcsec, 2s <QUIET>  Comp. 1 IDs-(7,20)
    EXPTIME  = 2
    LL_ID    = 7
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 20
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 66
    USABLE   = Y

STUDY
    STUDY_ID = 5
    TITLE_ID = 127
    OBS_PROG = O_HIVEL
    TITLE    = HIGH VELOCITY EVENT STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 1
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 5
    TITLE_ID = 127
    STUDYVAR = 13
    SV_DESC  = VARIATION 5, 50 RASTERS
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 66
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 1
        RAS_VAR  = 5
        N_REPEAT_R = 50
