DATATYPE = CDS STUDY DEFINITION
FILENAME = /mn/isis/u1/nilsbr/o_spot4_1.def
INSTRUME = CDS
DATE_CRE = 1997/11/06 08:13:01
END

LINELIST
    LL_ID    = 222
    DETECTOR = N
    LL_DESC  = O_SPOT4 lines
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.513
        GR_ORDER = 1
        CEN_PIX  = 355
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XVI
        WAVELNTH = 360.761
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 297
    DETECTOR = N
    DW_DESC  = Background,   7 lines. {0}  dex = (15,40) pixels <12484>
    W_WIDTH  = 15
    W_HEIGHT = 40
    VDS_BACK = 1
    LL_ID    = 222
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (348,432,15,40)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (419,432,15,40)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (603,432,15,40)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (733,432,15,40)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (751,552,15,40)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (855,552,15,40)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (990,432,15,40)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 152
    DETECTOR = N
    RAS_DESC = Slit(8x51),Posns(150,-)@(0,-) steps
    SLIT_NUM = 3
    XSTEP    = 0
    YSTEP    = 0
    NX       = 150
    NY       = 1

RASTER_VAR
    RAS_ID   = 152
    RAS_VAR  = 1
    RV_DESC  = (8x51) arcsec, 5s <QUIET>   Comp. 2 IDs-(222,297)
    EXPTIME  = 5
    LL_ID    = 222
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 297
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1315
    USABLE   = Y

STUDY
    STUDY_ID = 185
    TITLE_ID = 347
    OBS_PROG = O_SPOT4
    TITLE    = SUNSPOT VELOCITY FIELD AND LINE PROFILES   (JOP018)
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 152
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 185
    TITLE_ID = 347
    STUDYVAR = 1
    SV_DESC  = VAR. 1, 150 RASTER
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1315
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 152
        RAS_VAR  = 1
        N_REPEAT_R = 1
