DATATYPE = CDS STUDY DEFINITION
FILENAME = os_ar_9.def
INSTRUME = CDS
DATE_CRE = 2000/09/13 08:04:43
END

LINELIST
    LL_ID    = 355
    DETECTOR = N
    LL_DESC  = Active region oscillations
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = Fe XVI
        WAVELNTH = 335.425
        GR_ORDER = 1
        CEN_PIX  = 404
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = OV
        WAVELNTH = 629.505
        GR_ORDER = 1
        CEN_PIX  = 1008
        WAVEBAND = 2

DATAWIN
    DW_ID    = 496
    DETECTOR = N
    DW_DESC  = Background,   6 lines. {0}  dex = (30,110) pixels <25557>
    W_WIDTH  = 30
    W_HEIGHT = 110
    VDS_BACK = 1
    LL_ID    = 355
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = Fe_16_335_42                            
        WIN_DEF  = (389,517,30,110)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (608,397,30,110)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (738,397,30,110)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (853,517,30,110)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (954,397,30,110)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = WW_629_51                               
        WIN_DEF  = (993,397,30,110)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 61
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(200,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 200
    NY       = 1

RASTER_VAR
    RAS_ID   = 61
    RAS_VAR  = 9
    RV_DESC  = (4x220) arcsec, 14s <QUIET>  Comp. (8,2) IDs-(355,496)
    EXPTIME  = 14
    LL_ID    = 355
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 496
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 4000
    USABLE   = Y

STUDY
    STUDY_ID = 74
    TITLE_ID = 495
    OBS_PROG = OS_AR
    TITLE    = ACTIVE REGION OSCILLATIONS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 61
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 74
    TITLE_ID = 495
    STUDYVAR = 9
    SV_DESC  = VAR 1 - 6 LINES
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 4000
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 61
        RAS_VAR  = 9
        N_REPEAT_R = 1
