DATATYPE = CDS STUDY DEFINITION
FILENAME = /disk1/kucera/cds/pobs1_2_8.def
INSTRUME = CDS
DATE_CRE = 1997/04/14 18:06:56
END

LINELIST
    LL_ID    = 191
    DETECTOR = N
    LL_DESC  = Prominence Lines with Absorption 5
    N_LINES  = 16
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.66
        GR_ORDER = 1
        CEN_PIX  = 65
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Si VIII
        WAVELNTH = 319.83
        GR_ORDER = 1
        CEN_PIX  = 175
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Al XI
        WAVELNTH = 550.03
        GR_ORDER = 1
        CEN_PIX  = 317
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O IV
        WAVELNTH = 554.51
        GR_ORDER = 1
        CEN_PIX  = 355
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Ca X
        WAVELNTH = 557.77
        GR_ORDER = 1
        CEN_PIX  = 383
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Mg VIII/Fe X
        WAVELNTH = 335.3
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Ne VI
        WAVELNTH = 562.8
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = Si IX
        WAVELNTH = 345.12
        GR_ORDER = 1
        CEN_PIX  = 536
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Si X
        WAVELNTH = 347.4
        GR_ORDER = 1
        CEN_PIX  = 569
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Si IX
        WAVELNTH = 349.87
        GR_ORDER = 1
        CEN_PIX  = 604
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 12
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 13
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 14
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 15
        LINENAME = Si X/Mg X
        WAVELNTH = 624.85
        GR_ORDER = 1
        CEN_PIX  = 955
        WAVEBAND = 2
    LL_IND   = 16
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 261
    DETECTOR = N
    DW_DESC  = Background,  16 lines. {0}  dex = (22,120) pixels <22022>
    W_WIDTH  = 22
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 191
    N_WINS   = 20
    DW_IND   = 1
        WIN_NAME = Si_12_520_66                            
        WIN_DEF  = (54,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Si_8_319_83                             
        WIN_DEF  = (164,512,22,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Al_11_550_03                            
        WIN_DEF  = (306,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (344,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ca_10_557_77                            
        WIN_DEF  = (372,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = WW_335_30                               
        WIN_DEF  = (385,512,22,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (415,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Si_9_345_12                             
        WIN_DEF  = (525,512,22,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Si_10_347_40                            
        WIN_DEF  = (558,512,22,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_9_349_87                             
        WIN_DEF  = (593,512,22,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (599,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (729,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (797,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (851,512,22,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = WW_624_85                               
        WIN_DEF  = (944,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (986,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 20
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 14
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(30,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 14
    RAS_VAR  = 9
    RV_DESC  = (120x240) arcsec, 120s <ACTIVE>  Comp. 2 IDs-(191,261)
    EXPTIME  = 120
    LL_ID    = 191
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 261
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3785
    USABLE   = Y

STUDY
    STUDY_ID = 15
    TITLE_ID = 156
    OBS_PROG = POBS1_2
    TITLE    = PROMINENCE OBS PROGRAMME 1 PART 2
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 14
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 15
    TITLE_ID = 156
    STUDYVAR = 8
    SV_DESC  = VARIATION 4, ABSORPTION LINES
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3785
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 14
        RAS_VAR  = 9
        N_REPEAT_R = 1
