DATATYPE = CDS STUDY DEFINITION
FILENAME = prom_ion_60.def
INSTRUME = CDS
DATE_CRE = 2000/09/25 12:31:21
END

LINELIST
    LL_ID    = 357
    DETECTOR = N
    LL_DESC  = Prominence ionization
    N_LINES  = 10
    LL_IND   = 1
        LINENAME = HeI/CIII
        WAVELNTH = 537.8
        GR_ORDER = 1
        CEN_PIX  = 225
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ne IV
        WAVELNTH = 543.892
        GR_ORDER = 1
        CEN_PIX  = 277
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O IV
        WAVELNTH = 554.513
        GR_ORDER = 1
        CEN_PIX  = 368
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 439
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Ne V
        WAVELNTH = 572.331
        GR_ORDER = 1
        CEN_PIX  = 520
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O III
        WAVELNTH = 599.802
        GR_ORDER = 1
        CEN_PIX  = 755
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = He II
        WAVELNTH = 607.56
        GR_ORDER = 1
        CEN_PIX  = 821
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = O II
        WAVELNTH = 616.31
        GR_ORDER = 1
        CEN_PIX  = 896
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = O V
        WAVELNTH = 629.27
        GR_ORDER = 1
        CEN_PIX  = 1006
        WAVEBAND = 2

DATAWIN
    DW_ID    = 499
    DETECTOR = N
    DW_DESC  = Background,  10 lines. {0}  dex = (33,120) pixels <48660>
    W_WIDTH  = 33
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 357
    N_WINS   = 14
    DW_IND   = 1
        WIN_NAME = WW_537_80                               
        WIN_DEF  = (209,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ne_4_543_89                             
        WIN_DEF  = (261,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (352,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (423,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ne_5_572_33                             
        WIN_DEF  = (504,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (607,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_3_599_80                              
        WIN_DEF  = (739,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = He_2_607_56                             
        WIN_DEF  = (805,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = O_2_616_31                              
        WIN_DEF  = (880,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = O_5_629_27                              
        WIN_DEF  = (990,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 11
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(60,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 11
    RAS_VAR  = 66
    RV_DESC  = (240x240) arcsec, 30s <QUIET>  Comp. (8,2) IDs-(357,499)
    EXPTIME  = 30
    LL_ID    = 357
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 499
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 2257
    USABLE   = Y

STUDY
    STUDY_ID = 11
    TITLE_ID = 502
    OBS_PROG = PROM_ION
    TITLE    = PROMINENCE IONIZATION STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 11
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 11
    TITLE_ID = 502
    STUDYVAR = 60
    SV_DESC  = VAR 1 4" SLIT
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 2257
    ZONE_ID  = 1
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 11
        RAS_VAR  = 66
        N_REPEAT_R = 1
