DATATYPE = CDS STUDY DEFINITION
FILENAME = rt_mon_45.def
INSTRUME = CDS
DATE_CRE = 1998/01/18 15:37:21
END

LINELIST
    LL_ID    = 233
    DETECTOR = N
    LL_DESC  = RT Monitor
    N_LINES  = 5
    LL_IND   = 1
        LINENAME = Ne VI
        WAVELNTH = 562.711
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = HE I  584.3
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 611
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Fe XVI
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Mg IX  368.1
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = O V 629.73
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 311
    DETECTOR = N
    DW_DESC  = Background,   5 lines. {0}  dex = (21,120) pixels <10646>
    W_WIDTH  = 21
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 233
    N_WINS   = 9
    DW_IND   = 1
        WIN_NAME = Ne_6_562_71                             
        WIN_DEF  = (416,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (601,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (748,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (852,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (988,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 10
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 50
    RV_DESC  = (240x240) arcsec, 15s <QUIET>  Comp. 2 IDs-(233,311)
    EXPTIME  = 15
    LL_ID    = 233
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 311
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 2560
    USABLE   = Y

STUDY
    STUDY_ID = 10
    TITLE_ID = 358
    OBS_PROG = RT_MON
    TITLE    = RT MONITOR RASTER
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 10
    TITLE_ID = 358
    STUDYVAR = 45
    SV_DESC  = VERSION #1  MONITOR RT
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 2560
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        RAS_VAR  = 50
        N_REPEAT_R = 1
