DATATYPE = CDS STUDY DEFINITION
FILENAME = /disk1/thompson/database/export/sertscl2_33.def
INSTRUME = CDS
DATE_CRE = 1997/11/17 19:40:47
END

LINELIST
    LL_ID    = 219
    DETECTOR = N
    LL_DESC  = SERTS intercalibration linelist #3
    N_LINES  = 16
    LL_IND   = 1
        LINENAME = Mg VIII
        WAVELNTH = 314.226
        GR_ORDER = 1
        CEN_PIX  = 95
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Si VIII
        WAVELNTH = 315.902
        GR_ORDER = 1
        CEN_PIX  = 119
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Fe XIII
        WAVELNTH = 317.578
        GR_ORDER = 1
        CEN_PIX  = 143
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Si VIII
        WAVELNTH = 320.303
        GR_ORDER = 1
        CEN_PIX  = 182
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Fe XV
        WAVELNTH = 326.668
        GR_ORDER = 1
        CEN_PIX  = 273
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Cr XIII
        WAVELNTH = 328.348
        GR_ORDER = 1
        CEN_PIX  = 297
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Al X
        WAVELNTH = 333.322
        GR_ORDER = 1
        CEN_PIX  = 368
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Fe XVI
        WAVELNTH = 335.004
        GR_ORDER = 1
        CEN_PIX  = 392
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Mg VIII
        WAVELNTH = 338.651
        GR_ORDER = 1
        CEN_PIX  = 444
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Si IX
        WAVELNTH = 341.529
        GR_ORDER = 1
        CEN_PIX  = 485
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = Si IX
        WAVELNTH = 345.392
        GR_ORDER = 1
        CEN_PIX  = 540
        WAVEBAND = 1
    LL_IND   = 12
        LINENAME = Si X
        WAVELNTH = 347.57
        GR_ORDER = 1
        CEN_PIX  = 571
        WAVEBAND = 1
    LL_IND   = 13
        LINENAME = Si IX
        WAVELNTH = 349.328
        GR_ORDER = 1
        CEN_PIX  = 596
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = Fe XII
        WAVELNTH = 352.212
        GR_ORDER = 1
        CEN_PIX  = 637
        WAVEBAND = 1
    LL_IND   = 15
        LINENAME = Fe XIV
        WAVELNTH = 353.971
        GR_ORDER = 1
        CEN_PIX  = 662
        WAVEBAND = 1
    LL_IND   = 16
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2

DATAWIN
    DW_ID    = 293
    DETECTOR = N
    DW_DESC  = Background,  16 lines. {0}  dex = (25,120) pixels <20948>
    W_WIDTH  = 25
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 219
    N_WINS   = 20
    DW_IND   = 1
        WIN_NAME = Mg_8_314_23                             
        WIN_DEF  = (83,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Si_8_315_90                             
        WIN_DEF  = (107,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_13_317_58                            
        WIN_DEF  = (131,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Si_8_320_30                             
        WIN_DEF  = (170,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_15_326_67                            
        WIN_DEF  = (261,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Cr_13_328_35                            
        WIN_DEF  = (285,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Al_10_333_32                            
        WIN_DEF  = (356,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_16_335_00                            
        WIN_DEF  = (380,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_8_338_65                             
        WIN_DEF  = (432,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_9_341_53                             
        WIN_DEF  = (473,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Si_9_345_39                             
        WIN_DEF  = (528,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Si_10_347_57                            
        WIN_DEF  = (559,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Si_9_349_33                             
        WIN_DEF  = (584,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Fe_12_352_21                            
        WIN_DEF  = (625,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Fe_14_353_97                            
        WIN_DEF  = (650,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (796,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 20
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 38
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(30,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 38
    RAS_VAR  = 33
    RV_DESC  = (120x240) arcsec, 30s <QUIET>  Comp. 2 IDs-(219,293)
    EXPTIME  = 30
    LL_ID    = 219
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 293
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = H
    DURATION = 956
    USABLE   = Y

STUDY
    STUDY_ID = 44
    TITLE_ID = 342
    OBS_PROG = SERTSCL2
    TITLE    = SERTS CALIBRATION #2
    CATEGORY = C
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 38
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 44
    TITLE_ID = 342
    STUDYVAR = 33
    SV_DESC  = 16 LINE SET, 25 STEPS, LINE LIST #3
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 956
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 38
        RAS_VAR  = 33
        N_REPEAT_R = 1
