DATATYPE = CDS STUDY DEFINITION
FILENAME = test6_1_6.def
INSTRUME = CDS
DATE_CRE = 1996/03/15 13:47:14
END

LINELIST
    LL_ID    = 59
    DETECTOR = N
    LL_DESC  = TEST6 linelist with He II 304
    N_LINES  = 12
    LL_IND   = 1
        LINENAME = He 1 522.20
        WAVELNTH = 522.21
        GR_ORDER = 1
        CEN_PIX  = 77
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = FE 13  318.1
        WAVELNTH = 318.144
        GR_ORDER = 1
        CEN_PIX  = 175
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = He 1 537.03
        WAVELNTH = 537.07
        GR_ORDER = 1
        CEN_PIX  = 204
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = FE 14  334.2
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Ne 6 562.83
        WAVELNTH = 562.832
        GR_ORDER = 1
        CEN_PIX  = 424
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = MG  6  349.1
        WAVELNTH = 349.13
        GR_ORDER = 1
        CEN_PIX  = 602
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = He 1 584.33
        WAVELNTH = 584.341
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = O 3  599.59
        WAVELNTH = 599.552
        GR_ORDER = 1
        CEN_PIX  = 738
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = He II 303.78
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 806
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = MG  9  368.1
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 864
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = MG 10  624.9
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 955
        WAVEBAND = 2
    LL_IND   = 12
        LINENAME = O 5  629.73
        WAVELNTH = 629.741
        GR_ORDER = 1
        CEN_PIX  = 996
        WAVEBAND = 2

DATAWIN
    DW_ID    = 77
    DETECTOR = N
    DW_DESC  = Background,  12 lines.  dex = (15,120) pixels <17701>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 59
    N_WINS   = 16
    DW_IND   = 1
        WIN_NAME = He_1_522_21                             
        WIN_DEF  = (70,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_13_318_14                            
        WIN_DEF  = (168,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_537_07                             
        WIN_DEF  = (197,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (389,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ne_6_562_83                             
        WIN_DEF  = (417,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_6_349_13                             
        WIN_DEF  = (595,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = He_1_584_34                             
        WIN_DEF  = (601,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = O_3_599_55                              
        WIN_DEF  = (731,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (799,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (857,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (948,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = O_5_629_74                              
        WIN_DEF  = (989,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 3
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 3
    RAS_VAR  = 8
    RV_DESC  = (240x240) arcsec, 30s <QUIET>  Comp. 2 IDs-(59,77)
    EXPTIME  = 30
    LL_ID    = 59
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 77
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3915
    USABLE   = Y

STUDY
    STUDY_ID = 3
    TITLE_ID = 61
    OBS_PROG = TEST6_1
    TITLE    = NIS TEST STUDY: TEST6 PH.1
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 3
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 3
    TITLE_ID = 61
    STUDYVAR = 6
    SV_DESC  = 2X240 SLIT, 30S, TEST6 LINE LIST WITH HE II 304
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3915
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 3
        RAS_VAR  = 8
        N_REPEAT_R = 1
