DATATYPE = CDS STUDY DEFINITION
FILENAME = ~/cds_data/rasters/tranreg_19.def
INSTRUME = CDS
DATE_CRE = 1997/05/01 16:14:45
END

LINELIST
    LL_ID    = 181
    DETECTOR = N
    LL_DESC  = JOP 33 quick list with dens diags - 8 winds, 22 pix
    N_LINES  = 8
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.674
        GR_ORDER = 1
        CEN_PIX  = 65
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XII
        WAVELNTH = 338.26
        GR_ORDER = 1
        CEN_PIX  = 438
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = 
        WAVELNTH = 346.797
        GR_ORDER = 1
        CEN_PIX  = 560
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = 
        WAVELNTH = 348.343
        GR_ORDER = 1
        CEN_PIX  = 582
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Si X
        WAVELNTH = 356
        GR_ORDER = 1
        CEN_PIX  = 691
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 250
    DETECTOR = N
    DW_DESC  = Background,   8 lines. {0}  dex = (22,60) pixels <13485>
    W_WIDTH  = 22
    W_HEIGHT = 60
    VDS_BACK = 1
    LL_ID    = 181
    N_WINS   = 12
    DW_IND   = 1
        WIN_NAME = Si_12_520_67                            
        WIN_DEF  = (54,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_12_338_26                            
        WIN_DEF  = (427,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_346_80                               
        WIN_DEF  = (549,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_348_34                               
        WIN_DEF  = (571,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (599,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Si_10_356_00                            
        WIN_DEF  = (680,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (851,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (986,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 2
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(60,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 2
    RAS_VAR  = 29
    RV_DESC  = (120x120) arcsec, 10s <QUIET>  Comp. 2 IDs-(181,250)
    EXPTIME  = 10
    LL_ID    = 181
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 250
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 832
    USABLE   = Y

STUDY
    STUDY_ID = 32
    TITLE_ID = 241
    OBS_PROG = TRANREG
    TITLE    = TRANSITION REGION  2'X2'
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 32
    TITLE_ID = 241
    STUDYVAR = 19
    SV_DESC  = V.5 - JOP 33 QUICK + DENS, 8 WINDS, 22 PIX, 10S
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 832
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        RAS_VAR  = 29
        N_REPEAT_R = 1
