DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/user1/gdz/uclan_n1_1.def
INSTRUME = CDS
DATE_CRE = 1997/04/23 14:04:44
END

LINELIST
    LL_ID    = 174
    DETECTOR = N
    LL_DESC  = all NIS1 plus two windows in NIS2
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = First window
        WAVELNTH = 608.349
        GR_ORDER = 1
        CEN_PIX  = 815
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Second window 
        WAVELNTH = 627.398
        GR_ORDER = 1
        CEN_PIX  = 977
        WAVEBAND = 2

DATAWIN
    DW_ID    = 236
    DETECTOR = N
    DW_DESC  = Background, All NIS1  2 lines. {0}  dex = (70,45) pixels <8566>
    W_WIDTH  = 70
    W_HEIGHT = 45
    VDS_BACK = 1
    LL_ID    = 174
    N_WINS   = 7
    DW_IND   = 1
        WIN_NAME = WW_608_35                               
        WIN_DEF  = (780,430,70,45)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_627_40                               
        WIN_DEF  = (942,430,70,45)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = BB_NIS_1                                
        WIN_DEF  = (0,549,1024,45)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 135
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(25,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 25
    NY       = 1

RASTER_VAR
    RAS_ID   = 135
    RAS_VAR  = 1
    RV_DESC  = (100x90) arcsec, 50s <QUIET>  Comp. 2 IDs-(174,236)
    EXPTIME  = 50
    LL_ID    = 174
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 236
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1505
    USABLE   = Y

STUDY
    STUDY_ID = 166
    TITLE_ID = 296
    OBS_PROG = UCLAN_N1
    TITLE    = UCLAN CALIBRATION (NIS)
    CATEGORY = C
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 135
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 166
    TITLE_ID = 296
    STUDYVAR = 1
    SV_DESC  = VARIATION #1 100"X90" 50S
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1505
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 135
        RAS_VAR  = 1
        N_REPEAT_R = 1