DATATYPE = CDS STUDY DEFINITION
FILENAME = uvcs44w_12.def
INSTRUME = CDS
DATE_CRE = 1996/09/02 13:50:46
END

LINELIST
    LL_ID    = 106
    DETECTOR = N
    LL_DESC  = Off-limb detailed coronal study; 20 winds, 32 pix
    N_LINES  = 20
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.4
        GR_ORDER = 1
        CEN_PIX  = 65
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Mg VIII
        WAVELNTH = 313.016
        GR_ORDER = 1
        CEN_PIX  = 78
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg VIII
        WAVELNTH = 315.261
        GR_ORDER = 1
        CEN_PIX  = 110
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Al X
        WAVELNTH = 550
        GR_ORDER = 1
        CEN_PIX  = 317
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XIV
        WAVELNTH = 334.202
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Ca X
        WAVELNTH = 557.793
        GR_ORDER = 1
        CEN_PIX  = 384
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = Fe XII
        WAVELNTH = 338.481
        GR_ORDER = 1
        CEN_PIX  = 441
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Al X
        WAVELNTH = 568.222
        GR_ORDER = 1
        CEN_PIX  = 473
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = Si IX
        WAVELNTH = 342.129
        GR_ORDER = 1
        CEN_PIX  = 493
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Si IX
        WAVELNTH = 345
        GR_ORDER = 1
        CEN_PIX  = 534
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = Si X
        WAVELNTH = 347.25
        GR_ORDER = 1
        CEN_PIX  = 566
        WAVEBAND = 1
    LL_IND   = 12
        LINENAME = Si IX
        WAVELNTH = 349.495
        GR_ORDER = 1
        CEN_PIX  = 598
        WAVEBAND = 1
    LL_IND   = 13
        LINENAME = Fe XII
        WAVELNTH = 351.74
        GR_ORDER = 1
        CEN_PIX  = 630
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = Fe XIV
        WAVELNTH = 353.985
        GR_ORDER = 1
        CEN_PIX  = 662
        WAVEBAND = 1
    LL_IND   = 15
        LINENAME = Si X
        WAVELNTH = 356.23
        GR_ORDER = 1
        CEN_PIX  = 694
        WAVEBAND = 1
    LL_IND   = 16
        LINENAME = Fe XVI
        WAVELNTH = 360.75
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 17
        LINENAME = Fe XII
        WAVELNTH = 364.5
        GR_ORDER = 1
        CEN_PIX  = 812
        WAVEBAND = 1
    LL_IND   = 18
        LINENAME = Mg IX
        WAVELNTH = 368
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 19
        LINENAME = Mg X
        WAVELNTH = 624.817
        GR_ORDER = 1
        CEN_PIX  = 956
        WAVEBAND = 2
    LL_IND   = 20
        LINENAME = O V
        WAVELNTH = 629.621
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 141
    DETECTOR = N
    DW_DESC  = Background,  20 lines.  dex = (32,120) pixels <27186>
    W_WIDTH  = 32
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 106
    N_WINS   = 24
    DW_IND   = 1
        WIN_NAME = Si_12_520_40                            
        WIN_DEF  = (49,392,32,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_8_313_02                             
        WIN_DEF  = (62,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_8_315_26                             
        WIN_DEF  = (94,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Al_10_550_00                            
        WIN_DEF  = (301,392,32,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_14_334_20                            
        WIN_DEF  = (364,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Ca_10_557_79                            
        WIN_DEF  = (368,392,32,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Fe_12_338_48                            
        WIN_DEF  = (425,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Al_10_568_22                            
        WIN_DEF  = (457,392,32,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Si_9_342_13                             
        WIN_DEF  = (477,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_9_345_00                             
        WIN_DEF  = (518,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Si_10_347_25                            
        WIN_DEF  = (550,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Si_9_349_49                             
        WIN_DEF  = (582,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Fe_12_351_74                            
        WIN_DEF  = (614,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Fe_14_353_98                            
        WIN_DEF  = (646,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Si_10_356_23                            
        WIN_DEF  = (678,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = Fe_16_360_75                            
        WIN_DEF  = (742,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Fe_12_364_50                            
        WIN_DEF  = (796,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Mg_9_368_00                             
        WIN_DEF  = (846,512,32,120)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Mg_10_624_82                            
        WIN_DEF  = (940,392,32,120)
        WIN_FLAG = 0
    DW_IND   = 20
        WIN_NAME = O_5_629_62                              
        WIN_DEF  = (981,392,32,120)
        WIN_FLAG = 0
    DW_IND   = 21
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 22
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 23
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 24
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 8
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(60,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 8
    RAS_VAR  = 15
    RV_DESC  = (240x240) arcsec, 100s <QUIET>  Comp. 2 IDs-(106,141)
    EXPTIME  = 100
    LL_ID    = 106
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 141
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 6312
    USABLE   = Y

STUDY
    STUDY_ID = 8
    TITLE_ID = 231
    OBS_PROG = UVCS44W
    TITLE    = OFF-LIMB STUDY FOR CO-ORDINATION WITH UVCS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 8
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 8
    TITLE_ID = 231
    STUDYVAR = 12
    SV_DESC  = VARIATION 1, 32 PIX, 20 WINDS, 100S EXP
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 6312
    ZONE_ID  = 2
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 8
        RAS_VAR  = 15
        N_REPEAT_R = 1
